FSH_CALLDRIVER

Purpose

This routine allows FSDs to call a device driver's Extended Strategy entry point.

Calling Sequence

int far pascal FSH_CALLDRIVER(pPkt, hVPB, fControl) void far * pPkt; unsigned short hVPB; unsigned short fControl;

Where

pPkt is a pointer to device driver Extended strategy request packet.

hVPB is the volume handle for the source of I/O.

fControl is the bit mask of pop-up control actions:

Bit 0 off	indicates volume change pop-up desired
Bit 0 on	indicates no volume change pop-up
All other bits are reserved and must be zero.

Returns

If no error is detected, a zero error code is returned. If an error is detected, one of the following error codes is returned:

ERROR_VOLUME_CHANGED – is an indication that removable media volume change has occurred.

ERROR_INVALID_PARAMETER – the fControl flag word has reserved bits on.

Remarks

This routine should be called for any Extended strategy requests going to a drive that has removable media.

For a detailed description of the Extended Strategy request interface please see the OS/2 Version 2.0 Physical Device Driver Reference

FSH_CALLDRIVER may block.

Note: OS/2 does not validate input parameters. Therefore, an FSD should call FSH_PROBEBUF where appropriate.