Format of floppy format address field buffer entry (one per sector in track):

Offset	Size	Description
00h	BYTE	track number
01h	BYTE	head number (0-based)
02h	BYTE	sector number
03h	BYTE	sector size (00h=128 bytes, 01h=256 bytes, 02h=512, 03h=1024)