Note: This IBM PC BIOS API call is for DOS/Win16 personality only. Use Family API for portability.

Note: osFree Macro Library provides macros for most of functions

@VideoState

Brief

Return Video State

BIOS Interrupt

INT10H: H

Family API

fapi

Syntax

@VideoState

Parameters

none

Return