MFSH_INTERR - Internal Error

Purpose

Declare an internal error and halt the system.

Calling Sequence

int far pascal MFSH_INTERR(pcMsg, cbMsg) char far * pcMsg; unsigned short cbMsg;

Where

pcMsg is a pointer to the message text.

cbMsg is the length of the message text.

Returns

There are no error returns.

Remarks

This call should be used when an inconsistency is detected within the mini-FSD. This call does not return. An error message will be displayed and the system will be stopped. See the description of FSH_INTERR.